

making the total current through the voltage source (fowing out of it)



.

Thus, the equivalent resistance is



###### Solution to Exercise 3.15.2

Not necessarily, especially if we desire individual knobs for adjusting the gain and the cutof frequency.

###### Solution to Exercise 3.19.1

The ratio between adjacent values is about

